mqo2srf setting

Invert Normal:off
Unround All Vertex:off
RGB Color Format:on
Output DNM File:on
Output Only Complete DNM File:on
OutputOnly Visible Object:off
Unround Acute Vertex:off
Scale:1.0
Figure:6


DNMBuilder memo
1:ベースモデルを開く
open base model file by [Open]
2:リペイントモデルデータからPCKノードを読み込み上書きする
overwrite repaint model to base model by [Import PCKs from DNM file]
3:未使用PCKノードを削除する
dieting by [Delete non used PCK]
4:別名保存
save other name by [Save As]


//setfig setting
figures:0

//color blight set
0015 cabin_panel.srf
20002 inner_light_on.srf
10002 cabin_window_frame.srf without "230 230 230"
0016 cabin_frame.srf
0017~ seat.srf
0020 door_actuator.srf
0021 cabin_door.srf without "255 0 24"/"224 224 224"
0110 core_nacell.srf only "123 31 35"

//ZA change 3->1
body
cabin_door_skin
cabin_panel
cabin_frame

///difference by users customization or specification change

//aft cargo door change for wide size
back 0.9m polygon(need only mqo file)

//top storobe light position change for later production type
fwd 6.5m(need mqo file and dnm seting)